Jump to main content

##

# 2.65.9 MCPWM_ChannelSecondaryDutySet Function

## C

    void MCPWM_ChannelSecondaryDutySet(MCPWM_CH_NUM channel, uint16_t duty)

## Summary

Writes the secondary duty cycle value of given MCPWM channel

## Description

This function writes the secondary duty cycle value

## Precondition

MCPWM_Initialize() function must have been called first for the associated instance.

## Parameters

Param | Description
--- | ---
channel | MCPWM channel number
duty | duty cycle value which determines ON time of waveform

## Returns

None

## Example

    MCPWM_Initialize();
    MCPWM_Start();
    MCPWM_ChannelSecondaryDutySet(MCPWM_CH_0, 0x200);

## Remarks

In center-aligned asymmetric mode, this specifies the trailing edge of the ON time.