Jump to main content

##

# 2.110.41 USART_STOP Enum

## C

    /* Blocking, non-blocking and ring buffer mode */

    typedef enum
    {
        /* 1 bit stop bit */
        USART_STOP_1_BIT = SERCOM_USART_INT_CTRLB_SBMODE_1_BIT,

        /* 2 bit stop bit */
        USART_STOP_2_BIT = SERCOM_USART_INT_CTRLB_SBMODE_2_BIT,

        /* Force the compiler to reserve 32-bit memory for each enum */
        USART_STOP_INVALID = 0xFFFFFFFFU

    } USART_STOP;

## Summary

Defines the data type for the USART peripheral stop bits

## Description

This may be used in the SERCOMx_USART_SerialSetup API to change the stop bit configuration

## Remarks

None