Jump to main content

##

# 2.73.48 NVMCTRL_DATA_FLASH_START_ADDRESS Macro

## C

The start address of data flash varies based on device family. Refer to the generated header file for the actual start address value.

## Summary

Defines the start address of NVMCTRL DATA_FLASH.

## Description

This constant defines the start address of DATA_FLASH. It is recommended for the target application to use this constant in place hardcoded literals.

## Remarks

None.