Jump to main content

##

# 3.44.1 Analog Comparators (AC)

The Analog Comparator peripheral (AC) supports four individual comparators. Each comparator (COMP) compares the voltage levels on two inputs ('+' and '-' input pins of the comparator), and provides a digital output based on this comparison. Each comparator may be configured to generate interrupt requests and/or peripheral events upon several different combinations of input change.

The AC peripheral implements two pairs of comparators. Each pair can be set in window mode to compare a signal to a voltage range instead of a single voltage level.

## Using The Library

AC Peripheral library provides non-Blocking API's and they can be used to perform below functionalities on the AC peripheral.

- Initialize the AC

- Start comparison on a given comparator

- Swap inputs of a comparator

- Get status of a comparison operation

- Register a callback

## Library Interface

Analog Comparators peripheral library provides the following interfaces:

Functions

Name | Description
--- | ---
AC_Initialize | Initializes AC module of the device
AC_Start | Triggers a comparator to start comparison
AC_SwapInputs | Swap inputs of a comparator
AC_ChannelSelect | Selects the positive and negative inputs of a channel
AC_SetVddScalar | Sets VDDSCALER value of a comparator
AC_StatusGet | Returns comparison status of the AC
AC_CallbackRegister | Allows application to register callback with PLIB

Data types and constants

Name | Type | Description
--- | --- | ---
AC_CHANNEL | Enum | Identifies the AC output channel number
AC_POSINPUT | Enum | Identifies the positive inputs of a comparator channel
AC_NEGINPUT | Enum | Identifies negative inputs of a comparator channel
AC_CALLBACK | Typedef | Analog comparator callback function pointer