Jump to main content

##

# 1.1.1.24 mtch2120_getAKS

    MTCH2120_I2C_Status mtch2120_getAKS(uint8_t channel, uint8_t *value);

## Description:

This function reads AKS value from the MTCH2120 device memory via the I2C peripheral, according to the specified channel.

## Parameters:

Field | Type | Description
--- | --- | ---
channel | uint8_t | Channel Number to read the AKS value
value | uint8_t* | Buffer to store the read value

## Return:

MTCH2120_I2C_Status