Jump to main content

##

# 1.1.1.3 mtch2120_readFromMemory

    MTCH2120_I2C_Status mtch2120_readFromMemory(uint16_t memoryAddress, uint8_t *buffer, uint8_t length);

## Description:

This function reads data from the MTCH2120 device memory via the I2C peripheral, according to the specified length.

## Parameters:

Field | Type | Description
--- | --- | ---
memoryAddress | uint16_t | Address of the memory location
buffer | uint8_t * | Buffer to store the read value
length | uint8_t | Number of bytes to read

## Return:

MTCH2120_I2C_Status