Jump to main content

##

# 1.1.1.2 mtch2120_touchDeviceInit

    void mtch2120_touchDeviceInit(uint8_t address);

## Description:

This function initializes the host I2C driver and sets the MTCH2120 device address. It should be called whenever there is a need to change the device address.

## Parameters:

Field | Type | Description
--- | --- | ---
address | uint8_t | MTCH2120 device address

## Return:

void