Jump to main content

##

# 1 Harmony 3 Peripheral Library Application Examples for SAM D10 Family

Name | Description
--- | ---
EIC Interrupt | This example application demonstrates how to generate interrupt using the EIC on switch press and indicate it through an LED
PORT Polling | This example application demonstrate how to poll the switch input, and indicate the switch status using the LED
SERCOM USART Blocking | This example application demonstrates how to use the SERCOM peripheral in USART mode to transfer block of data in a blocking manner
SERCOM USART Interrupt | This example application demonstrates how to use the SERCOM peripheral in USART mode to transfer data in a non-blocking manner
Systick Periodic Interrupt | This example shows how to use the SysTick to generate periodic interrupts