Jump to main content

##

# 1.4.5.1 bootloader_XXX_Tasks Function

## C

    // XXX - Specifies the Bootloader Type
    void bootloader_XXX_Tasks(void)

## Summary

Starts bootloader execution.

## Description

This function can be used to start bootloader execution.

The function waits for application firmware from the Host devices (Host-PC/Embedded Host/Serial Memory) based on the bootloader running.

Once the complete application is received, programmed and verified successfully, it resets the device to jump into programmed application.

## Precondition

bootloader_Trigger() must be called to check for bootloader triggers at startup.

## Parameters

None

## Returns

None

## Example

    while(true)
    {
        bootloader_XXX_Tasks();
    }

## Remarks

For UART, I2C, SPI and CAN bootloaders this function runs in a infinite loop and it never returns