Jump to main content
1 Harmony 3 Driver and System Service Application Examples for SAM L22 Family
1.1 Console Debug System Service using UART
1.2 Console Debug System Service using USB
1.3 FAT Filesystem using NVM Media
1.4 FAT Filesystem using SD Card Media
1.5 FreeRTOS Basic
1.6 I2C Driver Asynchronous - Multi Client
1.7 SPI Driver Asynchronous - Multi Instance
1.8 Time System Service Multi-client
1.9 USART Driver Asynchronous - USART Echo
Microchip Information
Trademarks
Legal Notice
Microchip Devices Code Protection Feature