Jump to main content

# DRV_PLC_PHY_ID Enum

## G3 DRV_PLC_PHY_ID Enum

### C

    typedef enum {
        PLC_ID_HOST_DESCRIPTION_ID = 0x0100,
        PLC_ID_HOST_MODEL_ID  = 0x010A,
        PLC_ID_HOST_PHY_ID = 0x010C,
        PLC_ID_HOST_PRODUCT_ID = 0x0110,
        PLC_ID_HOST_VERSION_ID = 0x0112,
        PLC_ID_HOST_BAND_ID = 0x0116,
        PLC_ID_TIME_REF_ID = 0x0200,
        PLC_ID_PRODID = 0x4000,
        PLC_ID_MODEL,
        PLC_ID_VERSION_STR,
        PLC_ID_VERSION_NUM,
        PLC_ID_TONE_MASK,
        PLC_ID_TONE_MAP_RSP_DATA,
        PLC_ID_TX_TOTAL,
        PLC_ID_TX_TOTAL_BYTES,
        PLC_ID_TX_TOTAL_ERRORS,
        PLC_ID_TX_BAD_BUSY_TX,
        PLC_ID_TX_BAD_BUSY_CHANNEL,
        PLC_ID_TX_BAD_LEN,
        PLC_ID_TX_BAD_FORMAT,
        PLC_ID_TX_TIMEOUT,
        PLC_ID_RX_TOTAL,
        PLC_ID_RX_TOTAL_BYTES,
        PLC_ID_RX_RS_ERRORS,
        PLC_ID_RX_EXCEPTIONS,
        PLC_ID_RX_BAD_LEN,
        PLC_ID_RX_BAD_CRC_FCH,
        PLC_ID_RX_FALSE_POSITIVE,
        PLC_ID_RX_BAD_FORMAT,
        PLC_ID_ENABLE_AUTO_NOISE_CAPTURE,
        PLC_ID_TIME_BETWEEN_NOISE_CAPTURES,
        PLC_ID_DELAY_NOISE_CAPTURE_AFTER_RX,
        PLC_ID_RRC_NOTCH_ACTIVE,
        PLC_ID_RRC_NOTCH_INDEX,
        PLC_ID_NOISE_PEAK_POWER,
        PLC_ID_CRC_TX_RX_CAPABILITY,
        PLC_ID_RX_BAD_CRC_PAY,
        PLC_ID_CFG_AUTODETECT_IMPEDANCE,
        PLC_ID_CFG_IMPEDANCE,
        PLC_ID_ZC_PERIOD,
        PLC_ID_FCH_SYMBOLS,
        PLC_ID_TX_PAY_SYMBOLS,
        PLC_ID_RX_PAY_SYMBOLS,
        PLC_ID_RRC_NOTCH_AUTODETECT,
        PLC_ID_MAX_RMS_TABLE_HI,
        PLC_ID_MAX_RMS_TABLE_VLO,
        PLC_ID_THRESHOLDS_TABLE_HI,
        PLC_ID_THRESHOLDS_TABLE_LO,
        PLC_ID_THRESHOLDS_TABLE_VLO,
        PLC_ID_PREDIST_COEF_TABLE_HI,
        PLC_ID_PREDIST_COEF_TABLE_LO,
        PLC_ID_PREDIST_COEF_TABLE_VLO,
        PLC_ID_GAIN_TABLE_HI,
        PLC_ID_GAIN_TABLE_LO,
        PLC_ID_GAIN_TABLE_VLO,
        PLC_ID_DACC_TABLE_CFG,
        PLC_ID_RSV0,
        PLC_ID_NUM_TX_LEVELS,
        PLC_ID_CORRECTED_RMS_CALC,
        PLC_ID_RRC_NOTCH_THR_ON,
        PLC_ID_RRC_NOTCH_THR_OFF,
        PLC_ID_CURRENT_GAIN,
        PLC_ID_ZC_CONF_INV,
        PLC_ID_ZC_CONF_FREQ,
        PLC_ID_ZC_CONF_DELAY,
        PLC_ID_NOISE_PER_CARRIER,
        PLC_ID_SYNC_XCORR_THRESHOLD,
        PLC_ID_SYNC_XCORR_PEAK_VALUE,
        PLC_ID_SYNC_SYNCM_THRESHOLD,
        PLC_ID_TONE_MAP_RSP_ENABLED_MODS,
        PLC_ID_PPM_CALIB_ON,
        PLC_ID_SFO_ESTIMATION_LAST_RX,
        PLC_ID_PDC_LAST_RX,
        PLC_ID_MAX_PSDU_LEN_PARAMS,
        PLC_ID_MAX_PSDU_LEN,
        PLC_ID_RESET_STATS,
        PLC_ID_IC_DRIVER_CFG,
        PLC_ID_RX_CHN_EST_REAL,
        PLC_ID_RX_CHN_EST_IMAG,
        PLC_ID_TX_DISABLE,
        PLC_ID_TX_HIGH_TEMP_120,
        PLC_ID_TX_CANCELLED,
        PLC_ID_ZC_VALUE,
        PLC_ID_PDC_RX_LAST_RX,
        PLC_ID_PDC_ZC_TIME_LAST_RX,
        PLC_ID_PDC_ZC_PERIOD_LAST_RX,
        PLC_ID_PREAMBLE_NUM_SYNCP,
        PLC_ID_BAND,
        PLC_ID_CARRIER_DETECT,
        PLC_ID_END_ID,
    } DRV_PLC_PHY_ID;

### Summary

List of G3-PLC PHY IDs.

### Description

This data type contains every accessible object in G3-PLC PHY Information Base.

A detailed description of these objects is available in G3 DRV_PLC_PHY_IDs.

## PRIME DRV_PLC_PHY_ID Enum

### C

    typedef enum {
        PLC_ID_HOST_DESCRIPTION_ID = 0x0100,
        PLC_ID_HOST_MODEL_ID  = 0x010A,
        PLC_ID_HOST_PHY_ID = 0x010C,
        PLC_ID_HOST_PRODUCT_ID = 0x0110,
        PLC_ID_HOST_VERSION_ID = 0x0112,
        PLC_ID_HOST_BAND_ID = 0x0116,
        PLC_ID_TIME_REF_ID = 0x0200,
        PLC_ID_PRODID = 0x4000,
        PLC_ID_MODEL,
        PLC_ID_VERSION_STR,
        PLC_ID_VERSION_NUM,
        PLC_ID_CFG_AUTODETECT_IMPEDANCE,
        PLC_ID_CFG_IMPEDANCE,
        PLC_ID_ZC_TIME,
        PLC_ID_RX_PAY_SYMBOLS,
        PLC_ID_TX_PAY_SYMBOLS,
        PLC_ID_RSV0,
        PLC_ID_MAX_RMS_TABLE_HI,
        PLC_ID_MAX_RMS_TABLE_VLO,
        PLC_ID_THRESHOLDS_TABLE_HI,
        PLC_ID_THRESHOLDS_TABLE_LO,
        PLC_ID_THRESHOLDS_TABLE_VLO,
        PLC_ID_PREDIST_COEF_TABLE_HI,
        PLC_ID_PREDIST_COEF_TABLE_LO,
        PLC_ID_PREDIST_COEF_TABLE_VLO,
        PLC_ID_GAIN_TABLE_HI,
        PLC_ID_GAIN_TABLE_LO,
        PLC_ID_GAIN_TABLE_VLO,
        PLC_ID_DACC_TABLE_CFG,
        PLC_ID_CHANNEL_CFG,
        PLC_ID_NUM_TX_LEVELS,
        PLC_ID_CORRECTED_RMS_CALC,
        PLC_ID_CURRENT_GAIN,
        PLC_ID_ZC_CONF_INV,
        PLC_ID_ZC_CONF_FREQ,
        PLC_ID_ZC_CONF_DELAY,
        PLC_ID_SIGNAL_CAPTURE_START,
        PLC_ID_SIGNAL_CAPTURE_STATUS,
        PLC_ID_SIGNAL_CAPTURE_FRAGMENT,
        PLC_ID_SIGNAL_CAPTURE_DATA,
        PLC_ID_ENABLE_AUTO_NOISE_CAPTURE,
        PLC_ID_TIME_BETWEEN_NOISE_CAPTURES,
        PLC_ID_DELAY_NOISE_CAPTURE_AFTER_RX,
        PLC_ID_RRC_NOTCH_ACTIVE,
        PLC_ID_RRC_NOTCH_INDEX,
        PLC_ID_NOISE_PEAK_POWER,
        PLC_ID_RRC_NOTCH_AUTODETECT,
        PLC_ID_RRC_NOTCH_THR_ON,
        PLC_ID_RRC_NOTCH_THR_OFF,
        PLC_ID_TX_TOTAL,
        PLC_ID_TX_TOTAL_BYTES,
        PLC_ID_TX_TOTAL_ERRORS,
        PLC_ID_TX_BAD_BUSY_TX,
        PLC_ID_TX_BAD_BUSY_CHANNEL,
        PLC_ID_TX_BAD_LEN,
        PLC_ID_TX_BAD_FORMAT,
        PLC_ID_TX_TIMEOUT,
        PLC_ID_RX_TOTAL,
        PLC_ID_RX_TOTAL_BYTES,
        PLC_ID_RX_EXCEPTIONS,
        PLC_ID_RX_BAD_LEN,
        PLC_ID_RX_BAD_CRC_FCH,
        PLC_ID_RX_FALSE_POSITIVE,
        PLC_ID_RX_BAD_FORMAT,
        PLC_ID_NOISE_PER_CARRIER,
        PLC_ID_PPM_CALIB_ON,
        PLC_ID_ZC_PERIOD,
        PLC_ID_SYNC_THRESHOLDS,
        PLC_ID_NUM_CHANNELS,
        PLC_ID_MAX_NUM_CHANNELS,
        PLC_ID_PREDIST_COEF_TABLE_HI_2,
        PLC_ID_PREDIST_COEF_TABLE_LO_2,
        PLC_ID_PREDIST_COEF_TABLE_VLO_2,
        PLC_ID_NOISE_PER_CARRIER_2,
        PLC_ID_RESET_STATS,
        PLC_ID_IC_DRIVER_CFG,
        PLC_ID_RX_CHN_EST_REAL,
        PLC_ID_RX_CHN_EST_IMAG,
        PLC_ID_RX_CHN_EST_REAL_2,
        PLC_ID_RX_CHN_EST_IMAG_2,
        PLC_ID_TX_DISABLE,
        PLC_ID_TX_HIGH_TEMP_120,
        PLC_ID_TX_CANCELLED,
        PLC_ID_RX_CD_INFO,
        PLC_ID_SFO_ESTIMATION_LAST_RX,
        PLC_ID_END_ID,
    } DRV_PLC_PHY_ID;

### Summary

List of PRIME PLC PHY IDs.

### Description

This data type contains every accessible object in PRIME PLC PHY Information Base. A detailed description of these objects is available in PRIME DRV_PLC_PHY_IDs.

## Meters And More DRV_PLC_PHY_ID Enum

### C

    typedef enum {
        PLC_ID_HOST_DESCRIPTION_ID = 0x0100,
        PLC_ID_HOST_MODEL_ID  = 0x010A,
        PLC_ID_HOST_PHY_ID = 0x010C,
        PLC_ID_HOST_PRODUCT_ID = 0x0110,
        PLC_ID_HOST_VERSION_ID = 0x0112,
        PLC_ID_HOST_BAND_ID = 0x0116,
        PLC_ID_TIME_REF_ID = 0x0200,
        PLC_ID_PRODID = 0x4000,
        PLC_ID_MODEL,
        PLC_ID_VERSION_STR,
        PLC_ID_VERSION_NUM,
        PLC_ID_TX_TOTAL,
        PLC_ID_TX_TOTAL_BYTES,
        PLC_ID_TX_TOTAL_ERRORS,
        PLC_ID_TX_BAD_BUSY_TX,
        PLC_ID_TX_BAD_BUSY_CHANNEL,
        PLC_ID_TX_BAD_LEN,
        PLC_ID_TX_TIMEOUT,
        PLC_ID_TX_HIGH_TEMP_120,
        PLC_ID_TX_CANCELLED,
        PLC_ID_RX_TOTAL,
        PLC_ID_RX_TOTAL_BYTES,
        PLC_ID_RX_EXCEPTIONS,
        PLC_ID_RX_BAD_LEN,
        PLC_ID_RX_FALSE_POSITIVE,
        PLC_ID_RX_BAD_FORMAT,
        PLC_ID_RX_BAD_CRC_PAY,
        PLC_ID_RESET_STATS,
        PLC_ID_CRC_TX_RX_CAPABILITY,
        PLC_ID_CFG_AUTODETECT_IMPEDANCE,
        PLC_ID_CFG_IMPEDANCE,
        PLC_ID_ZC_PERIOD,
        PLC_ID_ZC_CONF_INV,
        PLC_ID_ZC_CONF_FREQ,
        PLC_ID_ZC_CONF_DELAY,
        PLC_ID_ZC_VALUE,
        PLC_ID_TX_PAY_SYMBOLS,
        PLC_ID_RX_PAY_SYMBOLS,
        PLC_ID_NUM_TX_LEVELS,
        PLC_ID_MAX_RMS_TABLE_HI,
        PLC_ID_MAX_RMS_TABLE_VLO,
        PLC_ID_THRESHOLDS_TABLE_HI,
        PLC_ID_THRESHOLDS_TABLE_LO,
        PLC_ID_THRESHOLDS_TABLE_VLO,
        PLC_ID_GAIN_TABLE_HI,
        PLC_ID_GAIN_TABLE_LO,
        PLC_ID_GAIN_TABLE_VLO,
        PLC_ID_DACC_TABLE_CFG,
        PLC_ID_IC_DRIVER_CFG,
        PLC_ID_TX_DISABLE,
        PLC_ID_RSV0,
        PLC_ID_CORRECTED_RMS_CALC,
        PLC_ID_CURRENT_GAIN,
        PLC_ID_SYNC_XCORR_THRESHOLD,
        PLC_ID_SYNC_XCORR_PEAK_VALUE,
        PLC_ID_PPM_CALIB_ON,
        PLC_ID_SFO_ESTIMATION_LAST_RX,
        PLC_ID_PREAMBLE_LEN_BYTES,
        PLC_ID_END_ID,
    } DRV_PLC_PHY_ID;

### Summary

List of Meters And More PHY IDs.

### Description

This data type contains every accessible object in Meters And More PHY Information Base.

A detailed description of these objects is available in Meters And More DRV_PLC_PHY_IDs.

Rev: G