Jump to main content

# DRV_PLC_PHY_CD_RX_STATE Enum

## C

    typedef enum {
      CD_RX_IDLE = 0,
      CD_RX_PREAMBLE_1_2 = 1,
      CD_RX_PREAMBLE_2_3 = 2,
      CD_RX_PREAMBLE = 3,
      CD_RX_HEADER = 4,
      CD_RX_PAYLOAD = 5,
    } DRV_PLC_PHY_CD_RX_STATE;

## Summary

List of Reception state values for Carrier Detect information.

## Description

This data type defines the list of reception state values for Carrier Detect information.

This is included in DRV_PLC_PHY_CD_INFO Struct.

Rev: G