Jump to main content

# 1.1.3.4.40 DRV_RF215_RX_INDICATION_OBJ Struct

## C

    typedef struct
    {
        /* RX time (PPDU start), referred to system 64-bit time counter */
        uint64_t                     timeIniCount;

        /* Pointer to received PSDU data */
        uint8_t*                     psdu;

        /* PPDU duration in system time counter units */
        uint32_t                     ppduDurationCount;

        /* PSDU length in bytes (including FCS) */
        uint16_t                     psduLen;

        /* RSSI in dBm */
        int8_t                       rssiDBm;

        /* Modulation scheme for the specific PHY type (FSK or OFDM) */
        DRV_RF215_PHY_MOD_SCHEME     modScheme;

        /* Correct FCS flag */
        bool                         fcsOk;

    } DRV_RF215_RX_INDICATION_OBJ;

## Summary

Defines the data reported in RF215 RX indication.

## Description

This data type defines the data reported in the RF215 receive indication (DRV_RF215_RX_IND_CALLBACK).

## Remarks

The `timeIni` parameter is only available if PHY TX/RX time support is enabled through MCC.

The `fcsOk` parameter is only available if Automatic Frame Check Sequence (FCS) is enabled through MCC.

Rev: G