Jump to main content

# SRV_PCOUP_Get_Config Function

## C

    SRV_PLC_PCOUP_DATA * SRV_PCOUP_Get_Config(void);

## Summary

Get the PLC PHY Coupling parameters.

## Description

This function allows to get the PLC PHY Coupling parameters. These parameters can be sent to the PLC device through PLC Driver PIB interface (DRV_PLC_PHY_PIBSet).

## Precondition

None.

## Parameters

None.

## Returns

- Pointer to SRV_PLC_PCOUP_DATA Struct, containing the PLC PHY Coupling parameters.

## Example

    SRV_PLC_PCOUP_DATA *pCoupValues;

    pCoupValues = SRV_PCOUP_Get_Config();

## Remarks

This function is only generated by MCC if the PLC driver uses Meters And More PHY.

If SRV_PCOUP_Set_Config function is used to set the PLC PHY Coupling parameters, this function is not needed.

Rev: G