Jump to main content

# 1.1.3.4.17 DRV_RF215_TX_HANDLE_INVALID Macro

## C

    #define DRV_RF215_TX_HANDLE_INVALID ((DRV_RF215_TX_HANDLE)(-1))

## Summary

Definition of an invalid transmission handle.

## Description

This is the definition of an invalid transmission handle. An invalid transmission handle is returned by DRV_RF215_TxRequest function if the request was not successful. It can happen due to invalid arguments, invalid driver handle, or lack of space in the queue.

## Remarks

None.

Rev: G