Jump to main content

# 1.1.3.4.18 DRV_RF215_TRX_ID Enum

## C

    typedef enum
    {
        RF215_TRX_ID_RF09  = 0,
        RF215_TRX_ID_RF24  = 1,

    } DRV_RF215_TRX_ID;

## Summary

Defines the available RF215 transceivers.

## Description

This data type defines the available RF215 transceivers (Sub-GHz and 2.4GHz). It is used in DRV_RF215_Open to identify the transceiver to be used by the client.

## Remarks

The availability of each transceiver is enabled through MCC.

Rev: G