Jump to main content

# 1.1.3.4.39 DRV_RF215_PHY_CFG_OBJ Struct

## C

    typedef struct
    {
        /* Channel center frequency F0 in Hz */
        uint32_t                     chnF0Hz;

        /* Channel spacing in Hz */
        uint32_t                     chnSpaHz;

        /* Minimum channel number */
        uint16_t                     chnNumMin;

        /* Maximum channel number */
        uint16_t                     chnNumMax;

        /* Minimum channel number (second range) (>0 for only one range) */
        uint16_t                     chnNumMin2;

        /* Maximum channel number (second range) (0 for only one range) */
        uint16_t                     chnNumMax2;

        /* Duration of Energy Detection for CCA (Clear Channel Assessment), in us */
        uint16_t                     ccaEdDurationUS;

        /* Energy Detection threshold for CCA, in dBm */
        int8_t                       ccaEdThresholdDBm;

        /* PHY type (FSK or OFDM) */
        DRV_RF215_PHY_TYPE           phyType;

        /* Configuration parameters for the specific PHY type (FSK or OFDM) */
        DRV_RF215_PHY_TYPE_CFG_OBJ   phyTypeCfg;

    } DRV_RF215_PHY_CFG_OBJ;

## Summary

Defines the data required to configure the RF215 PHY.

## Description

This data type defines the data required to configure the RF215 PHY.

This is a static PHY configuration, meaning that a RF215 device will only receive messages if the configuration is the same as in the transmitter.

## Remarks

None.

Rev: G