Jump to main content

# 1.1.2.4.23 DRV_G3_MACRT_SetBand Function

## C

    void DRV_G3_MACRT_SetBand( const DRV_HANDLE handle, MAC_RT_BAND band );

## Summary

Sets G3-PLC band.

## Description

This function allows a client to set the G3-PLC band.

## Precondition

DRV_G3_MACRT_Open must have been called to obtain a valid opened device handle.

## Parameters

Param | Description
--- | ---
handle | A valid open-instance handle, returned from the driver's open routine.
band | G3-PLC Band to set.

## Returns

None.

## Example

    DRV_HANDLE drvHandler;

    DRV_G3_MACRT_SetBand(drvHandler, G3_FCC);

## Remarks

None.

Rev: G