Jump to main content

# 1.2.8.4 Library Interface

RF PHY Serial library provides the following interfaces:

Functions

Name | Description
--- | ---
SRV_RSERIAL_GetCommand | Extracts command field from serial frame
SRV_RSERIAL_ParsePIB | Extracts PIB information from get/set PIB serial frame
SRV_RSERIAL_SerialGetPIB | Serializes a response to a get PIB command
SRV_RSERIAL_SerialSetPIB | Serializes a response to a set PIB command
SRV_RSERIAL_ParseTxMessageTrxId | Extracts the TRX identifier from SRV_RSERIAL_CMD_PHY_SEND_MSG serial frame
SRV_RSERIAL_ParseTxMessage | Extracts a RF frame to be transmitted from SRV_RSERIAL_CMD_PHY_SEND_MSG serial frame
SRV_RSERIAL_SetTxHandle | Sets the TX handle for the last TX request
SRV_RSERIAL_SerialRxMessage | Serializes a received RF frame and its related information
SRV_RSERIAL_SerialCfmMessage | Serializes the result of a RF transmitted frame

Data types and constants

Name | Type | Description
--- | --- | ---
SRV_RSERIAL_COMMAND | Enum | RF PHY Tester Tool commands enumeration

Rev: G