Jump to main content

# 1.1.2.4.44 MAC_RT_PHY_PIB Enum

## C

    typedef enum {
        PHY_PIB_PRODID = 0,
        PHY_PIB_MODEL,
        PHY_PIB_VERSION_STR,
        PHY_PIB_VERSION_NUM,
        PHY_PIB_TONE_MASK,
        PHY_PIB_TONE_MAP_RSP_DATA,
        PHY_PIB_TX_TOTAL,
        PHY_PIB_TX_TOTAL_BYTES,
        PHY_PIB_TX_TOTAL_ERRORS,
        PHY_PIB_TX_BAD_BUSY_TX,
        PHY_PIB_TX_BAD_BUSY_CHANNEL,
        PHY_PIB_TX_BAD_LEN,
        PHY_PIB_TX_BAD_FORMAT,
        PHY_PIB_TX_TIMEOUT,
        PHY_PIB_RX_TOTAL,
        PHY_PIB_RX_TOTAL_BYTES,
        PHY_PIB_RX_RS_ERRORS,
        PHY_PIB_RX_EXCEPTIONS,
        PHY_PIB_RX_BAD_LEN,
        PHY_PIB_RX_BAD_CRC_FCH,
        PHY_PIB_RX_FALSE_POSITIVE,
        PHY_PIB_RX_BAD_FORMAT,
        PHY_PIB_ENABLE_AUTO_NOISE_CAPTURE,
        PHY_PIB_TIME_BETWEEN_NOISE_CAPTURES,
        PHY_PIB_DELAY_NOISE_CAPTURE_AFTER_RX,
        PHY_PIB_RRC_NOTCH_ACTIVE,
        PHY_PIB_RRC_NOTCH_INDEX,
        PHY_PIB_NOISE_PEAK_POWER,
        PHY_PIB_CRC_TX_RX_CAPABILITY,
        PHY_PIB_RX_BAD_CRC_PAY,
        PHY_PIB_CFG_AUTODETECT_IMPEDANCE,
        PHY_PIB_CFG_IMPEDANCE,
        PHY_PIB_ZC_PERIOD,
        PHY_PIB_FCH_SYMBOLS,
        PHY_PIB_PAY_SYMBOLS_TX,
        PHY_PIB_PAY_SYMBOLS_RX,
        PHY_PIB_RRC_NOTCH_AUTODETECT,
        PHY_PIB_MAX_RMS_TABLE_HI,
        PHY_PIB_MAX_RMS_TABLE_VLO,
        PHY_PIB_THRESHOLDS_TABLE_HI,
        PHY_PIB_THRESHOLDS_TABLE_LO,
        PHY_PIB_THRESHOLDS_TABLE_VLO,
        PHY_PIB_PREDIST_COEF_TABLE_HI,
        PHY_PIB_PREDIST_COEF_TABLE_LO,
        PHY_PIB_PREDIST_COEF_TABLE_VLO,
        PHY_PIB_GAIN_TABLE_HI,
        PHY_PIB_GAIN_TABLE_LO,
        PHY_PIB_GAIN_TABLE_VLO,
        PHY_PIB_DACC_TABLE_CFG,
        PHY_PIB_RSV0,
        PHY_PIB_NUM_TX_LEVELS,
        PHY_PIB_CORRECTED_RMS_CALC,
        PHY_PIB_RRC_NOTCH_THR_ON,
        PHY_PIB_RRC_NOTCH_THR_OFF,
        PHY_PIB_CURRENT_GAIN,
        PHY_PIB_ZC_CONF_INV,
        PHY_PIB_ZC_CONF_FREQ,
        PHY_PIB_ZC_CONF_DELAY,
        PHY_PIB_NOISE_PER_CARRIER,
        PHY_PIB_SYNC_XCORR_THRESHOLD,
        PHY_PIB_SYNC_XCORR_PEAK_VALUE,
        PHY_PIB_SYNC_SYNCM_THRESHOLD,
        PHY_PIB_TONE_MAP_RSP_ENABLED_MODS,
        PHY_PIB_PPM_CALIB_ON,
        PHY_PIB_SFO_ESTIMATION_LAST_RX,
        PHY_PIB_PDC_TX_LAST_RX,
        PHY_PIB_MAX_PSDU_LEN_PARAMS,
        PHY_PIB_MAX_PSDU_LEN,
        PHY_PIB_RESET_STATS,
        PHY_PIB_PLC_IC_DRIVER_CFG,
        PHY_PIB_RX_CHN_EST_REAL,
        PHY_PIB_RX_CHN_EST_IMAG,
        PHY_PIB_TX_DISABLE,
        PHY_PIB_TX_HIGH_TEMP_120,
        PHY_PIB_TX_CANCELLED,
        PHY_PIB_ZC_VALUE,
        PHY_PIB_PDC_RX_LAST_RX,
        PHY_PIB_PDC_ZC_TIME_LAST_RX,
        PHY_PIB_PDC_ZC_PERIOD_LAST_RX,
        PHY_PIB_PREAMBLE_NUM_SYNCP
    } MAC_RT_PHY_PIB;

## Summary

List of G3-PLC PHY IDs.

## Description

This data type contains every accessible object in G3-PLC PHY Information Base.

A detailed description of these objects is available in G3 DRV_PLC_PHY_IDs.

Rev: G