Jump to main content

# 1.1.2.4.22 DRV_G3_MACRT_SetCoordinator Function

## C

    void DRV_G3_MACRT_SetCoordinator(const DRV_HANDLE handle);

## Summary

Enables G3-PLC coordinator capabilities.

## Description

This function allows a client to enable G3-PLC coordinator capabilities.

## Precondition

DRV_G3_MACRT_Open must have been called to obtain a valid opened device handle.

## Parameters

Param | Description
--- | ---
handle | A valid open-instance handle, returned from the driver's open routine.

## Returns

None.

## Example

    DRV_HANDLE drvHandler;

    DRV_G3_MACRT_SetCoordinator(drvHandler);

## Remarks

None.

Rev: G