Jump to main content

# 1.2.2.3 Configuring the Library

PLC PHY Sniffer Service is configured through MCC. Below is the figure of the MCC configuration window for PLC PHY Sniffer Service and brief description.

Figure 1-48.PLC PHY Sniffer Service Configuration Options

- PLC Profile specifies the PLC Profile and/or Working band used. Available options are:
  - PRIME: Shared profile for all channels, channel is later configured
  - G3 CEN-A: G3 Profile for Cenelec-A band
  - G3 CEN-B: G3 Profile for Cenelec-B band
  - G3 FCC: G3 Profile for FCC band

Note: As PLC PHY Sniffer Service is tightly linked to PLC PHY or MAC RT Driver, if PLC Profile is changed in PHY / MAC RT Driver Configuration, PHY Sniffer configuration is automatically updated to match the Profile selected in driver.

Rev: G