Jump to main content

# 1.2.4.4.5 SRV_PVDDMON_CheckWindow Function

## C

    bool SRV_PVDDMON_CheckWindow(void);

## Summary

Allows a client to check if the current ADC value is between correct threshold levels to be able to transmit through PLC.

## Description

Allows a client to check if the current ADC value is between correct threshold levels to be able to transmit through PLC. Threshold levels are obtained from the MCC.

## Precondition

Function SRV_PVDDMON_Start must have been called before calling this function.

## Parameters

None.

## Returns

True if the current ADC level is correct. Otherwise, false.

## Example

    if (SRV_PVDDMON_CheckWindow())
    {
        DRV_PLC_PHY_EnableTX(appData.drvPlcHandle, true);
        appData.pvddMonTxEnable = true;
    }
    else
    {
        DRV_PLC_PHY_EnableTX(appData.drvPlcHandle, false);
        appData.pvddMonTxEnable = false;
    }

## Remarks

None.

Rev: G