Jump to main content

# SRV_PCOUP_Set_Config Function

## C

    bool SRV_PCOUP_Set_Config(DRV_HANDLE handle, SRV_PLC_PCOUP_BRANCH branch);

## Summary

Set the PLC PHY Coupling parameters.

## Description

This function allows to set the PLC PHY Coupling parameters, using the PLC Driver PIB interface (DRV_PLC_PHY_PIBSet).

## Precondition

The PLC driver's open routine (DRV_PLC_PHY_Open) must have been called to obtain a valid opened device handle.

## Parameters

Param | Description
--- | ---
handle | A valid instance handle, returned from the PLC driver's open routine.

## Returns

- true:
  - Successful configuration
- false:
  - if there is an error when using the PLC driver PIB interface

## Example

    // 'handle', returned from DRV_PLC_PHY_Open or DRV_G3_MACRT_Open
    bool result;

    result = SRV_PCOUP_Set_Config(handle);

## Remarks

This function is only generated by MCC if the PLC driver uses Meters And More PHY.

Rev: G