Jump to main content

# 1.2.3.4.9 SRV_PSERIAL_COMMAND Enum

## C

    typedef enum
    {
        /* Get data configuration request */
        SRV_PSERIAL_CMD_PHY_GET_CFG = 0,
        /* Get data configuration response */
        SRV_PSERIAL_CMD_PHY_GET_CFG_RSP,
        /* Set data configuration request */
        SRV_PSERIAL_CMD_PHY_SET_CFG,
        /* Set data configuration response */
        SRV_PSERIAL_CMD_PHY_SET_CFG_RSP,
        /* Get command request */
        SRV_PSERIAL_CMD_PHY_CMD_CFG,
        /* Get command response */
        SRV_PSERIAL_CMD_PHY_CMD_CFG_RSP,
        /* Send message data */
        SRV_PSERIAL_CMD_PHY_SEND_MSG,
        /* Send message data response */
        SRV_PSERIAL_CMD_PHY_SEND_MSG_RSP,
        /* Receive message data */
        SRV_PSERIAL_CMD_PHY_RECEIVE_MSG

    } SRV_PSERIAL_COMMAND;

## Summary

List of PLC Serial Commands.

## Description

This enumeration defines the PLC commands used by PLC PHY Tester tool provided by Microchip.

Rev: G