Jump to main content

# 1.1.2.4.46 MAC_RT_TONE_MAP Struct

## C

    typedef struct {
        uint8_t toneMap[(MAX_PHY_TONE_GROUPS + 7) / 8];
    } MAC_RT_TONE_MAP;

## Summary

G3-PLC Tone Map.

## Description

This data type defines the Tone Map (dynamic notching) supported by G3-PLC spec.

Each bit corresponds to a sub-band of carriers and it indicates if such carriers carry message data (1) or pseudo-random data (0).

Rev: G