Jump to main content

# 1.1.2.4.48 MAC_RT_MOD_TYPE Enum

## C

    typedef enum {
        MAC_RT_MOD_ROBUST = 0x00,
        MAC_RT_MOD_BPSK = 0x01,
        MAC_RT_MOD_QPSK = 0x02,
        MAC_RT_MOD_8PSK = 0x03,
    } MAC_RT_MOD_TYPE;

## Summary

G3-PLC Modulation Types.

## Description

This data type defines the list of all types of modulation supported by G3-PLC spec.

## Remarks

Ordered from lower to higher data rate and from lower to higher required SNR (Signal to Noise Ratio): Robust BPSK, BPSK, QPSK, 8PSK.

Rev: G