Jump to main content

# 1.1.2.4.61 MAC_RT_SEGMENT_CONTROL Struct

## C

    typedef struct {
        /* Reserved */
        uint8_t reserved : 4;
        /* Tone Map Request */
        uint8_t toneMapRequest : 1;
        /* Contention Control */
        uint8_t contentionControl : 1;
        /* Channel Access Priority */
        uint8_t channelAccessPriority : 1;
        /* Last Segment Flag */
        uint8_t lastSegmentFlag : 1;
        /* Segment Count */
        uint16_t segmentCount : 6;
        /* Segment Length of MAC frame */
        uint16_t segmentLength : 10;
    } MAC_RT_SEGMENT_CONTROL;

## Summary

G3-PLC MAC Segment Control information.

## Description

This data type includes information related to the G3-PLC MAC segment control field.

## Remarks

For additional information, refer to the G3-PLC Specification.

Rev: G