Jump to main content

# SRV_PCOUP_Get_Default_Phy_Band Function

## C

    SRV_PLC_PCOUP_BRANCH SRV_PCOUP_Get_Default_Phy_Band( void );

## Summary

Get the default G3-PLC PHY band.

## Description

This function allows to get the G3-PLC PHY band used by default.

## Precondition

None.

## Parameters

None.

## Returns

Default G3-PLC PHY band.

## Example

    uint8_t plcPhyBand;

    plcPhyBand = SRV_PCOUP_Get_Default_Phy_Band();
    SRV_PCOUP_Set_Config(plcPhyBand);

## Remarks

This function is only generated by MCC if the PLC driver uses G3-PLC PHY.

Rev: G