Jump to main content

# 1.1.1.4.23 DRV_PLC_PHY_EXCEPTION Enum

## C

    typedef enum
    {
        /* SPI has detected an unexpected status, reset is recommended */
        DRV_PLC_PHY_EXCEPTION_UNEXPECTED_KEY,

        /* SPI critical error */
        DRV_PLC_PHY_EXCEPTION_CRITICAL_ERROR,

        /* Device has been reseted by Debugging tool */
        DRV_PLC_PHY_EXCEPTION_DEBUG,

        /* Device has been reseted */
        DRV_PLC_PHY_EXCEPTION_RESET

    } DRV_PLC_PHY_EXCEPTION;

## Summary

Defines the data type for PLC PHY Driver transfer errors.

## Description

This type is used to indicate the error (if any) of the last SPI transfer.

Rev: G