Jump to main content

# 1.2.3.4 Library Interface

PLC PHY Serial library provides the following interfaces:

Functions

Name | Description
--- | ---
SRV_PSERIAL_GetCommand | Extracts Command field from Serial frame
SRV_PSERIAL_ParseGetPIB | Extracts PIB field from SRV_PSERIAL_CMD_PHY_GET_CFG Serial frame
SRV_PSERIAL_SerialGetPIB | Serializes a response to a SRV_PSERIAL_CMD_PHY_GET_CFG command
SRV_PSERIAL_ParseSetPIB | Extracts PIB field from SRV_PSERIAL_CMD_PHY_SET_CFG Serial frame
SRV_PSERIAL_SerialSetPIB | Serializes a response to a SRV_PSERIAL_CMD_PHY_SET_CFG command
SRV_PSERIAL_ParseTxMessage | Extracts a PLC frame to be transmitted from SRV_PSERIAL_CMD_PHY_SEND_MSG Serial frame
SRV_PSERIAL_SerialRxMessage | Serializes a received PLC frame and its related information
SRV_PSERIAL_SerialCfmMessage | Serializes the result of a PLC transmitted frame

Data types and constants

Name | Type | Description
--- | --- | ---
SRV_PSERIAL_COMMAND | Enum | Defines the available PLC Serial commands

Rev: G