Jump to main content

# 1.1.3.4.38 DRV_RF215_PHY_TYPE_CFG_OBJ Union

## C

    typedef union
    {
        DRV_RF215_FSK_CFG_OBJ        fsk;
        DRV_RF215_OFDM_CFG_OBJ       ofdm;

    } DRV_RF215_PHY_TYPE_CFG_OBJ;

## Summary

Defines the data required to configure the RF215 FSK/OFDM PHY.

## Description

This data type defines the data required to configure the parameters associated to the corresponding RF215 PHY (FSK or OFDM).

This is a static PHY configuration, meaning that a RF215 device will only receive messages if the configuration is the same as in the transmitter.

Field description:

- fsk: FSK PHY configuration (see DRV_RF215_FSK_CFG_OBJ)
- ofdm: OFDM PHY configuration (see DRV_RF215_OFDM_CFG_OBJ)

## Remarks

None.

Rev: G