Jump to main content

# 1.1.2.4.66 MAC_RT_PHY_SNIFFER_HEADER Struct

## C

    typedef struct {
        /* SNIFFER_IF_PHY_COMMAND_G3_VERSION */
        uint8_t commandVersion;
        /* SNIFFER_VERSION */
        uint8_t snifferVersion;
        /* SNIFFER_PLC_G3 */
        uint8_t deviceVersion;
        /* ModType (high) + ModScheme (low) */
        uint8_t modTypeScheme;
        /* Tone Map */
        uint8_t toneMap[3];
        /* Number of symbols */
        uint16_t symbols;
        /* Link Quality Indicator */
        uint8_t lqi;
        /* Delimiter Type */
        uint8_t dt;
        /* Init time */
        uint32_t timeIni;
        /* End time */
        uint32_t timeEnd;
        /* RSSI */
        uint16_t rssi;
        /* AGC factor */
        uint16_t agcFactor;
        /* Data length */
        uint16_t dataLength;
    } MAC_RT_PHY_SNIFFER_HEADER;

## Summary

G3-PLC PHY sniffer parameters.

## Description

This data type includes information about G3-PLC PHY Sniffer packet.

## Remarks

This header is contained in the data reported by the callback set with DRV_G3_MACRT_PhySnifferCallbackRegister and it is compliant with Microchip Hybrid Sniffer tool.

Rev: G