Jump to main content

# 1.1.2.4.60 MAC_RT_FRAME_CONTROL Struct

## C

    typedef struct {
        /* Frame Type */
        uint16_t frameType : 3;
        /* Security Enable */
        uint16_t securityEnabled : 1;
        /* Frame pending */
        uint16_t framePending : 1;
        /* Ack Request */
        uint16_t ackRequest : 1;
        /* PAN ID Compression */
        uint16_t panIdCompression : 1;
        /* Reserved */
        uint16_t reserved : 3;
        /* Destination Addressing Mode */
        uint16_t destAddressingMode : 2;
        /* Frame Version  */
        uint16_t frameVersion : 2;
        /* Source Addressing Mode */
        uint16_t srcAddressingMode : 2;
    } MAC_RT_FRAME_CONTROL;

## Summary

G3 MAC Frame Control information.

## Description

This data type includes information related to the G3 MAC frame control field.

## Remarks

For additional information, refer to the G3 Specification.

Rev: G