Jump to main content

# 1.1.3.4.33 DRV_RF215_TX_RESULT Enum

## C

    typedef enum
    {
        RF215_TX_SUCCESS            = 0,
        RF215_TX_ERROR_UNDERRUN     = 1,
        RF215_TX_ABORTED            = 2,
        RF215_TX_BUSY_TX            = 3,
        RF215_TX_BUSY_RX            = 4,
        RF215_TX_BUSY_CHN           = 5,
        RF215_TX_TRX_SLEPT          = 6,
        RF215_TX_CANCEL_BY_RX       = 7,
        RF215_TX_TIMEOUT            = 8,
        RF215_TX_FULL_BUFFERS       = 9,
        RF215_TX_INVALID_LEN        = 10,
        RF215_TX_INVALID_DRV_HANDLE = 11,
        RF215_TX_INVALID_PARAM      = 12,
        RF215_TX_CANCELLED          = 13,

    } DRV_RF215_TX_RESULT;

## Summary

Defines the possible PHY transmission results.

## Description

This data type defines the list of possible PHY transmission results in RF215 driver.

## Remarks

None.

Rev: G