Jump to main content

# 1.1.3.4.31 DRV_RF215_PHY_CCA_MODE Enum

## C

    typedef enum
    {
        /* Energy above threshold only */
        PHY_CCA_MODE_1 = 0,

        /* Carrier sense only */
        PHY_CCA_MODE_2 = 1,

        /* Energy above threshold and carrier sense */
        PHY_CCA_MODE_3 = 2,

        /* ALOHA. CCA always reports idle medium */
        PHY_CCA_MODE_4 = 3,

        /* Transmit always, even if payload reception in progress */
        PHY_CCA_OFF    = 4,

    } DRV_RF215_PHY_CCA_MODE;

## Summary

Defines the available PHY Clear Channel Assessment (CCA) modes.

## Description

This data type defines the list of available PHY CCA modes in RF215 driver, as defined in 802.15.4. It is used as parameter in TX request.

## Remarks

None.

Rev: G