Jump to main content

##

# 1 MPLAB® Harmony 3 Ethernet Bootloader Application Examples

MPLAB® Harmony 3 is an extension of the MPLAB® ecosystem for creating embedded firmware solutions for Microchip 32-bit SAM and PIC® microcontroller and microprocessor devices. Refer to the following links for more information.

This repository contains the MPLAB® Harmony 3 Ethernet Bootloader application examples

Bootloader Library

Refer to Bootloader Library Help for understanding

- Bootloader framework
- How the Bootloader library works
- Bootloader library configurations
- Bootloader memory layout

Bootloader Examples

The following applications are provided to demonstrate the Ethernet bootloader

Name | Description
--- | ---
UDP Bootloader | This example application shows how to use the Bootloader Library to bootload an application using UDP protocol
UDP Live Update | This example application shows how to use the Bootloader Library as a Live Update application using UDP protocol on devices with Dual Bank Support