Jump to main content

# 2.1.4.38 DRV_MCMETROLOGY_MEASURE_TYPE Enum

## C

    typedefenum {
        MEASURE_V_AB = 0,
        MEASURE_V_BC,
        MEASURE_V_CA,
        MEASURE_V_AB_F,
        MEASURE_V_BC_F,
        MEASURE_V_CA_F,
        MEASURE_ACC_TO,
        MEASURE_ACC_T1,
        MEASURE_ACC_T2,
        MEASURE_FREQ,
        MEASURE_PT,
        MEASURE_PT_F,
        MEASURE_QT,
        MEASURE_QT_F,
        MEASURE_ENERGY,
        MEASURE_TYPE_NUM
    } DRV_MCMETROLOGY_MEASURE_TYPE;

## Summary

Identifies all types of generic measurements.

## Description

Values are calculated assuming: V_A is the first (lowest index) voltage channel defined, V_B is the second voltage channel defined, and V_C is the third voltage channel defined, where:

- V_AB = accumulated voltage to voltage (V) quantities between channels: V_A - V_B, fundamental + harmonics
- V_BC = accumulated voltage to voltage (V) quantities between channels: V_B - V_C, fundamental + harmonics
- V_CB = accumulated voltage to voltage (V) quantities between channels: V_C - V_A, fundamental + harmonics
- V_AB_F = accumulated voltage to voltage (V) quantities between channels: V_A - V_B, fundamental only
- V_BC_F = accumulated voltage to voltage (V) quantities between channels: V_B - V_C, fundamental only
- V_CB_F = accumulated voltage to voltage (V) quantities between channels: V_C - V_A, fundamental only
- ACC_TO = accumulated total energy according to the Pulse 0 Type selection (PC0_Type)
- ACC_T1 = accumulated total energy according to the Pulse 1 Type selection (PC1_Type)
- ACC_T2 = accumulated total energy according to the Pulse 2 Type selection (PC2_Type)
- FREQ = Frequency of fundamental harmonic
- PT = accumulated active power, fundamental + harmonics
- PT_F = accumulated active power, fundamental only
- QT = accumulated reactive power, fundamental + harmonics
- QT_F = accumulated reactive power, fundamental only
- ENERGY = accumulated total active energy

Rev: E