Jump to main content

# 2.1.4.36 DRV_MCMETROLOGY_CHANNEL_MEASURE_TYPE Enum

## C

    typedefenum {
        CHN_MEASURE_RMS = 0,
        CHN_MEASURE_RMS_F,
        CHN_MEASURE_MAX,
        CHN_MEASURE_FREQ,
        CHN_MEASURE_TYPE_NUM
    } DRV_MCMETROLOGY_CHANNEL_MEASURE_TYPE;

## Summary

Identifies all types of power channel measurements.

## Description

Values are calculated both including all harmonics and fundamental only (F added at the end of magnitude name), where:

- RMS = Voltage/Current RMS value, fundamental + harmonics
- RMS_F = Voltage/Current RMS value, fundamental only
- MAX = Maximum Voltage/Current value during the measurement interval
- FREQ = Frequency, fundamental only

Rev: E