Jump to main content

# 3.3.4.10 EMAFE_GetAllDataChannel Function

## C

    void EMAFE_GetAllDataChannel(uint8_t *pData);

## Summary

Get the last samples of all low-pass filters. Only supported if DMA is not enabled in EMAFE component in MCC configuration.

## Description

Get the last samples of all low-pass filters.

## Precondition

Low-pass filter must be enabled and DMA must be disabled.

## Parameters

Parameters | Description
--- | ---
pData | Pointer to data memory where data values will be written

## Returns

None.

## Example

    uint32_t samples[5];

    /* Get data from all channels */
    EMAFE_GetAllDataChannel((uint8_t *)samples);

## Remarks

None.

Rev: E