Jump to main content

# 1.1.4.17 DRV_METROLOGY_GetControlByDefault Function

## C

    DRV_METROLOGY_REGS_CONTROL * DRV_METROLOGY_GetControlByDefault (void);

## Summary

Get the pointer to the control registers defined by default through the Microchip Code Configurator (MCC) included in Harmony 3 framework.

## Description

After generating the Metrology Driver code through MCC, a struct data is defined as a constant. It includes all control registers obtained according to the MCC configuration established in the Harmony 3 project. The content of each control register is defined in `configuration.h` header file in the project.

## Parameters

None.

## Returns

Pointer to the control registers defined as the default configuration.

## Example

        DRV_METROLOGY_CONTROL *pSrc;

        pSrc = DRV_METROLOGY_GetControlByDefault();

## Remarks

None.

Rev: E