Jump to main content

# Meter ID Configuration Command

The Meter ID-related commands allow reading (IDR) or writing (IDW) the meter ID. The write command requires a password (“PIC” by default). The meter ID maximum length is limited to 6 characters.

    ; Write 123456 in the meter ID
    IDW[PIC](123456)
    Set Meter ID is ok

    ; Read the meter ID
    IDR
    Meter ID is:
    123456

    ; Write 1000AB in the meter ID
    IDW[PIC](1000AB)
    Set Meter ID is ok

    ; Read the meter ID
    IDR
    Meter ID is:
    1000AB

If Meter ID is not set before, the reading shown non-printable characters on the Console.

    ; Read the meter ID without being set before
    IDR
    Meter ID is:
    �������

Rev: E