Jump to main content

# 2.1.4.14 DRV_MCMETROLOGY_GetControlData Function

## C

    DRV_MCMETROLOGY_REGS_CONTROL * DRV_MCMETROLOGY_GetControlData (void);

## Summary

Get the pointer to the control registers of the metrology library application running on the second processor.

## Description

Control registers are acting as 32-bit metrology input control registers. For a detailed description of the control registers, refer to the `drv_metrology_regs.h` header file.

## Parameters

None.

## Returns

Pointer to the 32-bit metrology input control registers.

## Example

        /* Get Pointers to metrology data regions */
        app_metrologyData.pMetControl = DRV_MCMETROLOGY_GetControlData();
        app_metrologyData.pMetStatus = DRV_MCMETROLOGY_GetStatusData();
        app_metrologyData.pMetAccData = DRV_MCMETROLOGY_GetAccData();
        app_metrologyData.pMetHarData = DRV_MCMETROLOGY_GetHarData();

## Remarks

None.

Rev: E