Jump to main content

# 1.1.4.54 DRV_METROLOGY_HARMONICS_RMS Struct

## C

    typedefstruct {
        double Irms_A_m;
        double Irms_B_m;
        double Irms_C_m;
        double Irms_N_m;
        double Vrms_A_m;
        double Vrms_B_m;
        double Vrms_C_m;
    } DRV_METROLOGY_HARMONICS_RMS;

## Summary

Identifies the result of the harmonic analysis process.

## Description

Field description:

- Irms_A_m: RMS current value obtained as the result of last the harmonic analysis on channel A
- Irms_B_m: RMS current value obtained as the result of last the harmonic analysis on channel B
- Irms_C_m: RMS current value obtained as the result of last the harmonic analysis on channel C
- Irms_N_m: RMS current value obtained as the result of last the harmonic analysis on neutral channel
- Vrms_A_m: RMS voltage value obtained as the result of last the harmonic analysis on channel A
- Vrms_B_m: RMS voltage value obtained as the result of last the harmonic analysis on channel B
- Vrms_C_m: RMS voltage value obtained as the result of last the harmonic analysis on channel C

## Remarks

None.

Rev: E