Jump to main content

# 3.3.4.6 EMAFE_DisableFilter Function

## C

    void EMAFE_DisableFilter ( uint32_t filterMask );

## Summary

Disables the corresponding low-pass filter.

## Description

Disables the corresponding low-pass filter. filterMask can combine different filters.

## Precondition

None.

## Parameters

Parameters | Description
--- | ---
filterMask | Bit mask to indicate the low-pass filter to be disabled

## Returns

None.

## Example

    /* Init Decimation Filters */
    EMAFE_DisableFilter(EMAFE_MR_LPF_ON2_Msk | EMAFE_MR_LPF_ON4_Msk);

## Remarks

Table 3-8.Low Pass Filter Mask identifiers
Channel | Signal | Low Pass Filter Mask
--- | --- | ---
Channel 0 | Temperature Sensor | EMAFE_MR_LPF_ON0_Msk
Channel 1 | I1 | EMAFE_MR_LPF_ON1_Msk
Channel 2 | V1 | EMAFE_MR_LPF_ON2_Msk
Channel 3 | I2 | EMAFE_MR_LPF_ON3_Msk
Channel 4 | V2 | EMAFE_MR_LPF_ON4_Msk

Rev: E