Jump to main content

# 1.1.4.32 DRV_METROLOGY_CaptureDisableChannels Function

## C

    void DRV_METROLOGY_CaptureDisableChannels(uint8_t channelMask);

## Summary

Disable the channels to be captured.

## Description

Up to 7 channels of data may be captured at the same time. Only enabled channels are captured.

## Parameters

Parameters | Description
--- | ---
channelMask | Capture Disable Channel Mask

## Returns

None.

## Example

    DRV_METROLOGY_CaptureDisableChannels(CAPTURE_CHN_IB | CAPTURE_CHN_VB);

## Remarks

None.

Rev: E