Jump to main content

# 2.1.4.37 DRV_MCMETROLOGY_POWER_MEASURE_TYPE Enum

## C

    typedefenum {
        POW_MEASURE_P = 0,
        POW_MEASURE_P_F,
        POW_MEASURE_Q,
        POW_MEASURE_Q_F,
        POW_MEASURE_ANGLE,
        POW_MEASURE_TYPE_NUM
    } DRV_MCMETROLOGY_POWER_MEASURE_TYPE;

## Summary

Identifies all types of power source measurements.

## Description

Values are calculated both including all harmonics and fundamental only (F added at the end of magnitude name), where:

- P = Active power value, fundamental + harmonics
- P_F = Active power value, fundamental only
- Q = Reactive power value, fundamental + harmonics
- Q_F = Reactive power value, fundamental only
- ANGLE = Angle between the voltage and current vectors

Rev: E