Jump to main content

# 3.3.4.57 EMAFE_ADCGetSecurityControls Function

## C

    uint32_t EMAFE_ADCGetSecurityControls ( void );

## Summary

Get the security options of the analog system.

## Description

Get the security options of the analog system.

## Precondition

None.

## Parameters

None.

## Returns

Bit mask obtained from the secure options.

## Example

    secureOptions = EMAFE_ADCGetSecurityControls();

## Remarks

Secure Options | Description
--- | ---
EMAFE_ADC_SECURITY_SECRES_Msk | Restricted Access Security Level. When activated, this security level allows writing into the reserved configuration registers.
EMAFE_ADC_SECURITY_SECPRIV_Msk | Private Access Security Level. When activated, this security level bypasses internal FSM and allows the direct control of the analog cells. Note: When this security level is activated, the user must take care of not damaging analog IPs by activating a forbidden configuration.
EMAFE_ADC_SECURITY_SYS_RDY_DIS_Msk | System Ready Disable. When activated, the EMAFE ADC interface does not wait for the system ready signal be high to write into registers.

Rev: E