Jump to main content

# 1.1.4.48 DRV_METROLOGY_CALIBRATION_REFS Struct

## C

    typedef struct {
        double va;
        double ia;
        double aa;
        double vb;
        double ib;
        double ab;
        double vc;
        double ic;
        double ac;
        double in;
        double an;
        double vd;
        double avab;
        double avac;
        DRV_METROLOGY_CALIBRATION_MASK calMask;
    } DRV_METROLOGY_CALIBRATION_REFS;

## Summary

Specifies the all reference values used for the auto calibration process.

## Description

Field description:

- vx refers to the RMS voltage applied to the voltage input where x = A, B, C, D
- ix refers to the Rms current applied to the current input where x = A, B, C, N
- ax refers to the Angle between the voltage and current vectors where x = A, B, C, N, VAB, VAC
- calMask is a bitmask of the parameters to be calibrated

Rev: E