Jump to main content

# 1.1.4.31 DRV_METROLOGY_CaptureEnableChannels Function

## C

    void DRV_METROLOGY_CaptureEnableChannels(uint8_t channelMask);

## Summary

Enable the channels to be captured.

## Description

Up to 7 channels of data may be captured at the same time. Only selected channels are captured.

## Parameters

Parameters | Description
--- | ---
channelMask | Capture Channel Mask.

## Returns

None.

## Example

    DRV_METROLOGY_CaptureEnableChannels(CAPTURE_CHN_IA | CAPTURE_CHN_VA | CAPTURE_CHN_IB | CAPTURE_CHN_VB);

## Remarks

None.

Rev: E